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Standard (Non-Stock) Full Cylindrical Shaped
High-Temperature Ceramic Fiber Heaters (1100°C Construction Style
All Dimensions are in inches. Lead Locations A and C are approximate.
Complete the part number by adding the required lead location number.

Lead Location Part
A__C

10. |00, Watts | Volts Number
15 | 35 60| 120 | 15 05 |CFR30040]
20 | 50 00| 60 | 10 08 [CFR30050]
20 | 50 800 | 120 | 15 08 [CFR30060]
30 | 60 60| 120 | 10 08 |CPR30070)
30 | 60 1200 | 120 | 15 08 [CFR30080]
40 800 | 120 [ 10 10 |CFR30090)
40 1600 | 120 | 1S 10 [CFR30100]
50 000 | 120 | 10 10 |CFR30NE
50 2000 [ 120 | 15 10 |crr3on
60 1200 120 | 10 10 [CRR30130)
60 2400 | 120 | 15 10 [CFR30140]
60 3500 | 240 | 20 10 |cRR3ois0
80 1600 | 120 | 10 10 |CFR30160)
80 3100 | 240 | 15 10 |cRR30170)
100 2000 | 120 | 10 15 [CFR30190]
100 3900 [ 240 | 1515 | crrio200
100 5900 | 240 | 20 15 [CFR30210
120 4700 | 240 | 15 15 |CFR3023]
120 7100 | 240 | 20 15 [CFR30240]
140 8200|240 [ 20 15

CFR30260]
7100 | 200 | 15 20 |crraoas0 )/
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All Dimensions are in inches. Lead Locations A, B and C are approximate.
Complete the part number by adding the required lead location number.

- Load Location | Part
ID. OD. L Watts Voits A B C | Number
20 60 60 200 60 |10 10 10 |CFRS003]
20 60 120 400 120 |15 10 10 [CFRS004C]
20 60 180 600 120 |20 10 10 [CFRS00S]
20 60 240 800 240 |20 10 10 | CFRS0060]
3575 60 350 60 10 1S 10 [CFRS0070]
350 75120 700 120 |15 1S 10 [ CFRS008C]
50 90 60 500 60 |10 15 10 |CFRS0IIC]
50 90 120 1000 120 |15 15 10 [CFRS0120
50 90 180 1500 240 |20 15 10 [CFRSO13T
50 90 240 2000 240 |20 15 10 | CFRS0C]
50 90 300 2500 240 (25 15 10 |CFRS0IS(]
50 90 360 3000 240 |25 15 10 |CFRS016(]
65 105 60 650 120 |10 20 10 |CFRS0170)
65105 120 1300 | 240 | 15 20 10 | CFRS0IS]
65105 180 1950 | 240 (20 20 10 | CFRS0I90]
65 105 240 2600 | 240 |20 20 10 | CFRS0200]
80 120 120 1600 240 | 1S 20 10 [CFRs023(]
80 120 180 2400 240 |20 20 10 [CFRS024(]
80 120 240 3200 240 |20 20 10 [CFRS0250]
80 120 360 4800 240 |25 20 10 [CFRS0270]
100 140 120 2000 | 240 |15 20 10 | CFRS028(]
100 | 140 180 3000 240 |20 20 10 |CFRS0290]
100 140 240 4000 | 240 |20 20 10 | CFRS030(]
120 160 120 2400 | 240 |15 20 10 | CFRS033(]
120 160 180 3600 | 240 |20 20 10 | CFRSOM[]
120160 240 4800 | 240 [20 20 10 | CFRS03SC]
150 190 120 3000 | 240 |15 20 10 | CFRS038(]
150 190 180 4500 ' 240 |20 20 10 | CFRS0390]
150 190 240 6000 | 240 |20 20 10 | CFRS040(]
150 190 300 7500 | 240 |25 20 10 |CFRS041]

\U50 190 360 9000 240 |25 20 10 | CFRs0420]/





